**320 Overhead or Underground Meter Base**

|  |  |
| --- | --- |
| TYPE | Ringless Meter Socket |
| APPLICATION | Meter Socket |
| STANDARD | UL Listed Type 3R |
| VOLTAGE RATING | 600 Volts Alternating Current |
| AMP RATING | 320 Continuous Ampere |
| PHASE | 3 Phase |
| FREQUENCY RATING | 60 Hertz |
| # OF MAIN BREAKERS | 0 |
| CABLE ENTRY | OH, Underground and Side Wireway |
| TERMINAL | 3/8 inch stud |
| INSULATION | Glass Polyester |
| MOUNTING | Surface Mount |
| MATERIAL | G90 Galvanized Steel w/powder coat finish |
| # OF JAWS | 7 Terminal |
| BYPASS PROVISION | Lever Bypass |
| # OF METER POSITIONS | 1 |
| EQUIPMENT GROUND | Grounding Stud |
| HUB/CLOSING PLATE | Large Closing Plate |
| # OF RECEPTACLES | 0 |
| HEIGHT | 34.125 IN |
| LENGTH | 6.5 IN |
| WIDTH | 19 IN |