**125 Overhead or Underground Meter Base**

|  |  |
| --- | --- |
| TYPE | Ringless Meter Socket |
| APPLICATION | Meter Socket |
| STANDARD | UL Listed Type 3R |
| VOLTAGE RATING | 600 Volts Alternating Current |
| AMP RATING | 125 Continuous Ampere |
| PHASE | Single |
| FREQUENCY RATING | 60 Hertz |
| # OF MAIN BREAKERS | 0 |
| CABLE ENTRY | Overhead or Underground |
| TERMINAL | Lay in |
| INSULATION | Glass Polyester |
| MOUNTING | Surface Mount |
| MATERIAL | G90 Galvanized Steel w/powder coat finish |
| # OF JAWS | 4 terminal |
| BYPASS PROVISION | No Bypass |
| # OF METER POSITIONS | 1 |
| EQUIPMENT GROUND | Triplex Ground |
| HUB/CLOSING PLATE | Small Hub Opening |
| LOAD SIDE WIRE RANGE | 6-2/0 AWG |
| LINE SIDE WIRE RANGE | 6-2/0 AWG |
| # OF RECEPTACLES | 0 |
| HEIGHT | 11.5 IN |
| LENGTH | 3.313 IN |
| WIDTH | 8 IN |